

LOGO [Insert Company Logo Here]

COMPANY - COSHH ASSESSMENT
CHERRY LAUREL
	Assessment status
	Document control

	Hazard-specific assessment - confirm site exposure
	Reference: AOS-BIO-22 | Version: 1.0

	Applies to
	Assessment date: ____ / ____ / ______

	Arboriculture, forestry, grounds maintenance and outdoor work
	Review date: ____ / ____ / ______


1. Hazard identification
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Identification photographs retained from supplied SBust reference.
	Hazard
	Details

	Common name
	Cherry Laurel

	Organism / botanical name
	Prunus laurocerasus

	Where encountered
	Gardens, estates, parks, schools, hedges and woodland planting.

	Persons potentially exposed
	Employees, climbers, grounds staff, trainees/apprentices, contractors, visitors and the public if controls fail


2. Warning symbols
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Poisonous material


Naturally occurring biological or plant hazard; chemical CLP pictograms normally do not apply. The symbols used here are workplace warning and PPE symbols.
3. Exposure routes and health effects
	Exposure routes
	Potential harm

	Ingestion; inhalation of dust/fumes from cutting or confined accumulations of freshly chipped material
	Plant tissues contain cyanogenic compounds; ingestion can be poisonous; Fresh chipped material in an enclosed chip box may create a dangerous atmosphere


	Initial risk
	Residual risk after controls
	Health surveillance

	High
	Low
	Review need with competent occupational-health advice where exposure is regular, sensitisation is possible or symptoms are reported.


4. Required controls
Check client/site information and survey for this hazard before work. Record presence, extent, affected tasks and controls in the SSRA.
Do not enter or work inside a chip box/confined space containing fresh laurel chip
Keep chip compartments ventilated and manage as a confined-space/DSEAR-type atmospheric risk where relevant
Prevent ingestion; minimise dust and keep people/animals from arisings
Use tools or mechanical methods to avoid direct contact where reasonably practicable. Maintain an exclusion zone where material could spread, project or expose others.
Do not eat, drink or smoke in the exposure area. Keep contaminated PPE/equipment away from vehicles, climbing equipment and welfare areas.
Provide soap-and-water handwashing and clean/decontaminate tools, boots and PPE without spreading contamination.
Stop work and inform the Team Leader if the hazard is unexpected, identification is uncertain or controls cannot be achieved.
5. Mandatory / task-selected PPE
	[image: ]
Protective gloves
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Eye protection
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Suitable RPE
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Coveralls / covered skin
	[image: ]
Hand washing


PPE selection must match the task and exposure level. RPE is only effective when correctly selected; tight-fitting RPE requires face-fit testing, a clean-shaven seal, training, inspection and replacement. PPE does not replace avoidance, mechanical control or exclusion.
6. Emergency and first aid action
Move to fresh air immediately if unwell; do not enter to rescue without confined-space arrangements
Call 999 for breathing difficulty, collapse or suspected poisoning
Report the exposure, injury, symptoms or near miss promptly and record the site, task, time and suspected agent.
Call 999 for breathing difficulty, collapse, severe allergic reaction, seizures, serious poisoning or other life-threatening symptoms.
7. Training, hygiene and review
	Required check
	Record

	Team trained to recognise the hazard and briefed on controls
	Yes / No

	Site-specific assessment and exclusion arrangements completed
	Yes / No / N/A

	PPE, washing, decontamination and first aid available
	Yes / No / N/A

	Specialist advice / occupational health required
	Yes / No / N/A

	Assessor / date / review date
	________________________________________


Review at least annually and sooner after an incident, symptom report, new guidance, change in work method, evidence of spread/contamination or concern that controls are ineffective.


[COMPANY NAME] – COSHH Assessment – Biological Hazards (Generic) – ARB-COSHH-03
Version: [VERSION]   Date Issued: [DATE]   Review Date: [REVIEW DATE]
Not controlled when printed.
image1.jpeg




image2.jpeg




image3.png




image4.png




image5.png




image6.png




image7.png




image8.png




