LOGO [Insert Company Logo Here]

COMPANY: Climbing / Aerial Rescue Plan
1. Site & Document Details
Site / Project: 
Client / Principal Contractor: 
Location: 
Date: 
Review Date: 
2. Purpose
This rescue plan sets out the procedures to be followed in the event of an emergency involving a tree climber. It ensures that a prompt and effective rescue can be carried out, minimising risk to the casualty and rescuers. This plan must be briefed to all relevant operatives prior to climbing operations commencing.
3. Legislative & Guidance References
• Work at Height Regulations 2005
• Provision and Use of Work Equipment Regulations 1998 (PUWER)
• AFAG / FISA Guidance (current editions)
4. Competence Requirements
All climbers must be appropriately trained and competent for the tasks being undertaken. A designated aerial rescuer must be present on site at all times when climbing operations are carried out. The aerial rescuer must be competent and equipped to carry out a rescue.
5. Rescue Equipment
The following rescue equipment must be available and immediately accessible:
• Climbing and rescue kit
• Additional ropes and lowering devices
• First aid kit (including trauma / bleed control where provided)
• Communication devices (mobile phone / radio)
6. Emergency Scenarios & Rescue Procedures
6.1 Conscious Casualty in Tree
The designated aerial rescuer will access the casualty using safe climbing techniques. The casualty will be reassured and secured before being lowered to the ground in a controlled manner.
6.2 Unconscious Casualty in Tree
Dial 999 immediately and inform emergency services of a casualty suspended at height. The aerial rescuer will access the casualty as quickly and safely as possible, secure them using appropriate rescue techniques, and lower them to the ground. First aid will be administered until emergency services arrive.
6.3 Casualty Injured by Cutting Equipment
Stop all work immediately and make the area safe. Dial 999 if injuries are serious. Apply first aid, including bleed control if required, and carry out an aerial rescue if the casualty is unable to descend unaided.
6.4 Suspension Trauma
If a casualty is suspended in their harness, rescue must be carried out as a priority. Where possible, instruct the casualty to move their legs to promote circulation. Once lowered, keep the casualty in a seated position and monitor until emergency services arrive.
7. Emergency Contacts
Emergency Services: 999
Site Contact / Supervisor: 
Company Emergency Contact:
8. Nearest Hospital
Name: 
Address: 
Postcode: 
9. Briefing Confirmation
I confirm that this Climbing / Aerial Rescue Plan has been briefed to all relevant operatives prior to climbing operations commencing.
	Name
	Signature
	Date
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